QUANTITIES HAVE CHANGED AS PART OF THIS ADDENDUM- Line item #1 has been reduced. 2 new line items have been added before the Add Alternative items with clearer descriptions.

USE THIS ADDENDUM TO SUBMIT PRICING IN YOUR BID RESPONSE.

-Vendor must be an authorized ViewSonic K-12 reseller.

-Installations must be completed before January 20, 2023 work being done during second shift.

-A mandatory meeting will start at **Staples High School** at 3:00 PM on October 27, 2022. All vendors will be provided a detailed specification including pictures of new installations. If vendors have additional questions and wish to continue with a walkthrough, we will then proceed to all schools.

-All cables must be terminated in wall plate and must be neatly enclosed in wire mold or wall. In-wall wiring preferred when possible.

-ALL disconnected previously used equipment, cables, and wall plates, etc. must remain intact and left at the schools in designated locations.

-ALL in-wall or ceiling cable must be riser rated, except for installations in Long Lots School and Coleytown Elementary, which must be plenum-rated.

-Vendor must provide a spreadsheet of installed equipment with room #, and ViewSonic Board serial #.

**-If ViewSonic Board fails and requires replacement within warranty period (5 years), vendor is required to provide physical removal/replacement services within 5 business days of receipt of equipment. (Westport will handle support case and hardware shipping arrangements.)**

Questions regarding this bid specification may be directed to:

Natalie Carrignan, Director of Technology

ncarrignan@westportps.org 203-341-1217

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  | **Qty** | **Unit****Price** | **Extended****Price** |
| 1 | **Replace existing SMART Board with ViewSonic  IFP7550-E1 (w. Conen mount)**- Mounting of new vendor supplied ViewSonic IFP7550-E1-Two year extended warranty (5-years total) **IFP-EW-70-02****-**Provide and install Conen adjustable stand, part # **SCETAWL** (or equivalent- attached product details to bid response)-Provide and install cable package (HDMI, USB 2.0+ w. Cat5+ Extender where necessary)-Install Wall Plate - HDMI, and USB Pass Through - Cables to Go Part #**39702** (or equivalent- attached product details to bid response)-Uninstall all unused equipment, leave in room for WPS tech to remove-Remove or blank plate unused boxes and wall plates | 21 |  |  |
| 2 | **Replace existing SMART Board with ViewSonic IFP7550-E1 (w. Build out Brackets)** -Mounting of new vendor supplied ViewSonic IFP7550-E1-Two year warranty extension (total 5 years) **IFP-EW-70-02**-Provide and install build out brackets-Provide and install cable package (HDMI, USB 2.0+ w. Cat5+ Extender where necessary)-Install Wall Plate - HDMI, and USB Pass Through - Cables to Go Part #**39702,** (or equivalent- attached product details to bid response)-Uninstall all unused equipment, leave in room for WPS tech to remove-Remove or blank plate unused boxes, and wall plates | 14 |  |  |
| 3 | **Replace existing SMART Board with ViewSonic IFP7550-E1 (no Build out Brackets)** -Mounting of new vendor supplied ViewSonic IFP7550-E1-Two year warranty extension (total 5 years) **IFP-EW-70-02**-Provide and install build out brackets-Provide and install cable package (HDMI, USB 2.0+ w. Cat5+ Extender where necessary)-Install Wall Plate - HDMI, and USB Pass Through - Cables to Go Part #**39702,** (or equivalent- attached product details to bid response)-Uninstall all unused equipment, leave in room for WPS tech to remove-Remove or blank plate unused boxes, and wall plates | 1 |  |  |
| 4 | **Replace existing SMART Board with ViewSonic  IFP7550-E2 (portable stand. (LLS)** **-**-Two year extended warranty (5-years total) **IFP-EW-70-02****-** Install Viewsonic board onto stand | 1 |  |  |
| 5 | **Install NEW ViewSonic  IFP7550-E2 (portable stand. (CES portable)** **-**-Two year extended warranty (5-years total) **IFP-EW-70-02****-** Install Viewsonic board onto stand | 1 |  |  |
| 6 | **Add alternate for additional location, w/ Item 2 Specifications (BMS)** | 1 |  |  |
| 7 | **Add alternate for additional location, w/ Item 2 Specifications (BMS)** | 4 |  |  |

VENDOR NAME:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_